**Description of incident *(No company names or site locations)***

|  |
| --- |
| A crew was adding 2 parts of line for a total of 6 parts to a 135T crane.  After the load was lifted, the guide pin cut the line causing the load and the block to fall to the ground.  • Fortunately, no one was injured but there was damage to the crane and the customer’s property. |

**Contributing Factors/Cause(s) *(if any)***

|  |
| --- |
| Potential complacency in performing what is considered a routine activity. |

**Root Cause(s)**

|  |
| --- |
| The line was run over the guide pin instead of under it. |

**Other Potential Causes *(if any)***

|  |
| --- |
| 1. Deteriorated/missing slip-resistant tape was not identified on daily inspection |

**Corrective Actions or Recurrence Controls**

|  |
| --- |
| After completing a task, double check the work. |

**Lessons Learned**

|  |
| --- |
| Complacency can have serious consequences, including loss of life.  Always Inspect your work. |

**Photos or Sketches**

|  |
| --- |
|  |